|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Potential**  **Hazard** | **How might people be**  **harmed** | **Those**  **At Risk** | **Control Measures** | **Risk**  **Rating** |
| Display Vehicles | Collisions with pedestrians Collisions with structures | All | * Competent licenced drivers * All cars must be Road worthy or be transported on an approved trailer * Locking petrol caps used wherever feasible * Once cars are positioned engines will not be re-started until all public are out of the field and organisers give permission. * All Display vehicles will be insured with their own liability insurance as part of that policy | MED |
| Vehicle Movement on Show field | Collisions between vehicles Collisions with pedestrians Collisions with structures | All | * No vehicle movement on the show field from 11.30am to 4.00pm * One way system within show field. * 10mph speed limit on show field. * No reversing without banksman * Wide entrances on to and off the field * No vehicle movement whatsoever in the field while any public are around the cars | MED |
| Vehicle movement on the main road | Collisions between vehicles Collisions with pedestrians | All | * Experienced marshals to control traffic on to and off the show field. | LOW |
| Fire | Fire within Gazebo causes injury, panic, smoke inhalation | All | * No smoking inside Gazebo * Reduce presence of combustibles * Place Fire extinguishers at critical points * Sufficient emergency fire exits * Fire Emergency Plan | LOW |
| Collapse of Structures | Structures not erected properly | All | * Structures to be erected by competent trained ELMOC persons | LOW |
| Adverse  weather | High winds on Gazebo banners and flags. etc. | All | * If winds exceed 25mph Gazebo to be evacuated and stewards to direct visitors to a safe location. * ELMOC Stewards will safely gazebo banners and flags before they become a problem | LOW |
| Slips Trips & Falls | Muddy conditions; Cables; hosepipes; guy ropes etc. | All | * Monitor conditions on the day and use warning tape for significant risks.(eg guy ropes) | LOW |
| Electricity & Gas | Electric shock from portable generators and wiring.  Gas leak from heaters or ovens | All | * ELMOC have no requirement for Electrical or Gas items within their display | LOW |
| Crowding | Crushing  Unable to escape in an  emergency | All | * ELMOC Members only in Gazebo and no more than 20 members at any one time | LOW |
| Aggressive or Disruptive Behaviour |  | All | * ELMOC Committee members to monitor the situation and if necessary call for police assistance | LOW |